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	MAINTENANCE ACTION PLAN & SCOPE OF WORK FOR FIVE YEARS MAJOR OVERHAUL 
	RIG NO
	D.P.3

	
	
	LOCATION
	BOURI FIELD 

	
	
	DATE OF START
	06-10-2026

	
	
	Estimate maintenance time 
	4 WEEKS 



OFFSHORE RIG

D.P.3

NWD MAINTENANCE SCOPE OF WORK FOR FIVE YEARS MAJOR OVERHAUL  

	
	Equipment name ( type , model , serial No)
	Serial NO
	Summary / scope of work
	Maint crew
	Date start
	Date finish

	1
	Crown blocks sheaves
	
	NDT inspection of sheaves , shaft , support beams , brackets & check bearing & seals ( replace bearing & seals if required )  
	 
	
	

	2
	Fast line sheave
	
	NDT inspection of sheaves , shaft , support beams , brackets & check bearing & seals ( replace bearing & seals if required )  
	
	
	

	3
	Travelling blocks
	
	NDT inspection of sheaves ,center pin , cross head , side plates , pins , check bearing & seals ( replace bearings & seals if required )
	
	
	

	4
	Draw works
	
	Inspection of bearing clearance & condition 
	
	
	

	5
	Draw works brake mechanism
	
	NDT inspection of brake bands, brake linkage & equalizer bar. 
	
	
	

	6
	Draw works air system
	
	Need to check sir hoses , fitting & drill console control valves 
	
	
	

	7
	Air winch#1
	
	NDT inspection of foundation , sheaves and swivels , control valve if required 
	
	
	

	8
	Air winch#2
	
	NDT inspection of foundation , sheaves and swivels , control valve if required
	
	
	

	9
	Mud pump# 1
	
	Check bearings , cross head clearance add shims as required , lubricating system , cooling system & checkup roller chain input drive replace if required
	
	
	

	10
	Mud pump# 2


	
	Check bearings , cross head clearance add shims as required , lubricating system , cooling system & checkup roller chain input drive replace if required
	
	
	

	11
	Mud agitators
	
	To be check & replace some parts if required 
	
	
	

	12
	Rotary table
	
	Inspection, gear box & check the brake & clearance.
	
	
	

	13
	Rotary table gear box 
	
	To be check , adjustment  & replace some parts if required
	
	
	

	14
	Swivel
	
	NDT inspection of foundation , control valve if required 
	
	
	

	15
	Main HYD unite
	
	To be check & replace some parts if required
	
	
	

	16
	Bop fork lift
	
	General check up 
	
	
	

	17
	Engine NO1 # CAT 399
	
	General checkup 
	
	
	

	18
	Engine NO2 # CAT 399
	
	General checkup
	
	
	

	19
	Engine NO3 # CAT 399
	
	General checkup
	
	
	

	20
	Engine NO4 # CAT 399
	
	General checkup
	
	
	

	21
	Emergency GEN 399
	
	General checkup
	
	
	

	22
	Air compressor A
	
	general checkup
	
	
	

	23
	Air compressor B
	
	general checkup
	
	
	

	24
	Air compressor C
	
	general checkup
	
	
	

	25
	Cold start compressor


	
	general checkup
	
	
	

	26
	Koomy unite
	
	check nitrogen for all bottles of accumulator & check bladder & valves 
	
	
	

	Electrical equipment scope of work 

	1
	Instrumentation
	
	general checkup
	
	
	

	2
	BOP electrical control system 
	
	Clean contacts tips of triplex pump power contactor, tighten bolts and weirs terminal, check alarm box and replace indicator lights, 
	
	
	

	3
	D.C motor
	
	Check brushes, brushes holder, pressure and flow switch, clean the commutate and tighten power and control terminal.
	
	
	

	4
	Shall shaker
	
	Check all motor connection and wire terminal, clean control panel, push button station. 
	
	
	

	5
	Mud agitators 
	
	Check motors, start/stop stations and indication lights.
	
	
	

	6
	Main & EM-Generators 
	
	Merger power phases tighten connection bolts General cleaning and check em-generator Starter batteries.
	
	
	

	7
	Motor control circuit  M.C.C
	
	Meggaring M.C.C checks tighten connection, change induction lights and change meters as required.
	
	
	

	8
	Mud pumps remote control panel 
	
	Check and clean throttle and selector switch, tighten loses terminal block screws replaced indicator lights. 
	
	
	

	9
	Drill console
	
	Clean hand throttle and assignment selector switch, tighten terminal, and start/stop station.  
	
	
	

	10
	SCR system 
	
	Disassembly SCR cell .check, clean thyrestors, clean power & field contactor, tighten loos connection. 
	
	
	

	11
	Normal light system 
	
	Check the lights in the rig, cleaning & repair if required .
	
	
	

	12
	Air dryer 
	
	Check & service 
	
	
	

	13
	Main switch board  
	
	Apply current injection test for SCR & generators C .barker
	
	
	

	14
	Overhead travelling electric hoist “engine room 
	
	Check & service
	
	
	

	15
	Mini breakers
	
	Install new  MINIATURE circuit breaker need to be replaced "function test failure"


	
	
	

	16
	Top drive control system 
	
	Troubleshooting operation control logic make a temporary link for top drive control logic until repair or upgrade crown gas detector system                                            
	
	
	


