

**المواصفات الفنية**

**TECHNICAL SPECIFICATION**

**عطاء رقم BID NO. NWD-TC-2023-T-50-20**

|  |  |  |  |
| --- | --- | --- | --- |
| **No.** | **Qty.** | **Uoi.** | **Description.** |
| 1 | 1 | EA | |  | | --- | | **Power swivel model S-120 swivel unit** | | **Manufactured by Bowen or Logan** | | with a 3.5 S-120 swivel head powered | | by Cat engine. Unit is mounted on new oil | | Field skid; with air control panel, hydraulic | | Reel and winch, Bowen Model S3.5 120 | | tons swivel with the following design | | Features; torque 8100ft lbs | | speed 150 RPM, circulating pressure 5000psi | | Static load rating 120 tons | | Equipped with Cat diesel engine | | Electric starter, 12 volts alternator, | | Battery, battery box and radiator | | Remote air control panel has removal | | Pedestal with air control valve | | Forward and reverse, w/100 ft long hoses | | Hydraulic winch to pull back swivel | | 3 each parts books and manuals | | COC Certificate | |