

**المواصفات الفنية**

**TECHNICAL SPECIFICATION**

**عطاء رقم BID NO. NWD-TC-2023-T-50-20**

|  |  |  |  |
| --- | --- | --- | --- |
| **No.** | **Qty.** | **Uoi.** | **Description.** |
| 1 | 1 | EA |

|  |
| --- |
| **Power swivel model S-120 swivel unit** |
| **Manufactured by Bowen or Logan**  |
| with a 3.5 S-120 swivel head powered |
| by Cat engine. Unit is mounted on new oil  |
| Field skid; with air control panel, hydraulic  |
| Reel and winch, Bowen Model S3.5 120 |
| tons swivel with the following design  |
| Features; torque 8100ft lbs |
| speed 150 RPM, circulating pressure 5000psi |
| Static load rating 120 tons |
| Equipped with Cat diesel engine |
| Electric starter, 12 volts alternator,  |
| Battery, battery box and radiator |
| Remote air control panel has removal  |
| Pedestal with air control valve |
| Forward and reverse, w/100 ft long hoses |
| Hydraulic winch to pull back swivel  |
| 3 each parts books and manuals |
| COC Certificate |

 |